Jump to main content

# View OR directors

Unisphere supports the display of OR director information.

## Prerequisites

See Roles and associated permissions to determine the user roles that can perform this task.

## About this task

For a storage system running PowerMaxOS 10 (6079), a new OR emulation has been added to replace all previous Open System Front End and RDF emulations (see Understanding OR Directors). The system hardware view has an OR DIRECTORS tab, a BE DIRECTORS tab, an EF DIRECTORS tab, and an EM DIRECTORS tab.

## Steps

1. Select a storage system running PowerMaxOS 10 (6079).
2. Select System > Hardware.
3. Click the OR Directors tab.

   The OR Directors list view opens. A filtered list view is displayed. Virtual ports are filtered out of the view. The following properties display (unfiltered view):

   Director | Director name.
   Port | Port number.
   Director Status | Director status.
   Port Status | Indicates whether the port is online or offline.
   Enabled Protocol | Indicates the protocol setting (SCSI FC, iSCSI, NVMe/FC, NVMe/TCP, RDF FC, or RDF GIGE).
   Port Type | Indicates if the port type is Fibre or GigE.
   Speed GB/sec | Indicates negotiated speed.
   Alerts | Director alert status, as indicated by icon color: One or more fatal alerts One or more critical alerts, with none higher One or more warning alerts, with none higher One or more informational alerts, with none higher No alerts
   Virtual | Indicates if the port is virtual.
   Port ID | Port ID.

   To see more information about the details and performance of a director, select a director and click . The properties that are displayed depend on the protocols that are enabled on the director. Some of the following properties and controls are environment-specific and therefore may appear in a different order or not at all.

   Director | Director name.
   Port | Port ID.
   Type | Type.
   Director Status | Director status.
   Port Status | Indicates whether the port is online or offline.
   Director Connection Status | Indicates if the director is connected.
   Protocols | Number of associated protocols. Clicking the number next to Protocols displays information about the protocol properties and performance of the protocols.
   Port Topology | Port topology.
   Volumes | Number of associated volumes. Clicking the number next to Volumes displays information about the properties of the volumes.
   WWN | WWN
   Fibre Channel Loop ID | Fibre channel loop ID.
   Negotiated Speed (Gb/sec) | Negotiated speed in gigabits per second.
   Max Speed (Gb/sec) | Maximum speed in gigabits per second.
   Cloud Port | Indication if port is a cloud port.
   MAC Address | MAC address
   IP Interfaces | Number of IP interfaces. Clicking the number next to IP Interfaces displays the list of IP interfaces.
   NVMe/TCP Endpoints | Number of attached NVMe/TCP endpoints. Clicking the number next to NVMe/TCP Endpoints displays the list of NVMe/TCP endpoints.
   iSCSI Endpoints | Number of attached iSCSI endpoints. Clicking the number next to iSCSI Endpoints displays the list of iSCSI endpoints.
   IPv4 Address | IPv4 Address
   IPv6 Address | IPv6 Address
   IPv6 Prefix | IPv6 Prefix
   RDF Groups | Number of SRDF groups. Clicking the number next to RDF Groups displays the list of SRDF groups.
   RDF Software Compression Support | Indicates if SRDF software compression is supported.
   RDF Hardware Compression Support | Indicates if SRDF hardware compression is supported.
   Synchronous I/O Percent | Synchronous I/O percent
   Asynchronous I/O Percent | Asynchronous I/O percent
   Copy I/O Percent | Copy I/O percent
   VCM State | Indicator of VCM state (Enabled or Disabled)
   ACLX | Indicator of ACLX (Enabled or Disabled)
   Common Serial Number | Indicator of common serial number (Enabled or Disabled)
   Unique WWN | Indicator of unique WWN (Enabled or Disabled)
   Init Point to Point | Indicator of init point to point (Enabled or Disabled)
   Volume Set Addressing | Indicator of volume set addressing (Enabled or Disabled).
   VNX Attached | Indicator of VNX attached (Enabled or Disabled)
   Avoid Reset Broadcast | Indicator of Avoid Reset Broadcast (Enabled or Disabled)
   Negotiate Reset | Indicator of negotiate reset (Enabled or Disabled).
   Enable Auto Negotiate | Indicator of enable auto negotiate (Enabled or Disabled).
   Environ Set | Indicator of environ set (Enabled or Disabled).
   Disable Q Reset on UA | Indicator of disable Q reset on UA (Enabled or Disabled)
   Soft Reset | Indicator of soft reset (Enabled or Disabled)
   SCSI3 | Indicator of SCSI3 (Enabled or Disabled)
   SCSI Support1(OS2007) | Indicator of SCSI Support1(OS2007) (Enabled or Disabled)
   No Participating | Indicator of no participating (Enabled or Disabled)
   SP2 Protocol Version | Indicator of SP2 Protocol Version (Enabled or Disabled)
   HP3000 Mode | Indicator of HP3000 mode (Enabled or Disabled)
   Sunapee | Indicator of Sunapee (Enabled or Disabled)
   Siemens | Indicator of Siemens (Enabled or Disabled)
   Sequent | Indicator of Sequent (Enabled or Disabled)
   Server on AS400 | Indicator of the state of the server on AS400 (Enabled or Disabled)
   Enable AS400 | Indicator of Enable AS400 (Enabled or Disabled)
   Open VMS | Indicator of open VMS (Enabled or Disabled)
   Open Replicator Maximum Ceiling(MB) | Indicator of open replicator maximum ceiling in MB
   Open Replicator Ceiling (%) | Indicator of open replicator ceiling (as a percentage)
   Open Replicator Actual Ceiling (MB) | Indicator of open replicator actual ceiling in MB

   Performance information is also displayed in the Performance tab.

   The following controls are available:

   - Online—Sets the port to be online.
   - Offline—Sets the port to be offline.
   - Manage Protocol— Manage Protocol for OR director
   - Set Port Attributes— Set director port attributes
   - Set ORS Ceiling— Set Open Replicator ceiling
   - CPU I/O Setting— Set CPU I/O resource distribution
   - SRDF GigE> Create IP Interface— Configure an IP interface for OR or RE ports
   - SRDF GigE > Modify IP Interface— Configure an IP interface for OR or RE ports
   - SRDF GigE > Delete IP Interface— Configure an IP interface for OR or RE ports

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com