Jump to main content

# Create an IP route

Unisphere provides monitoring and management for Non-Volatile Memory Express (NVMe/TCP) directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

## About this task

This topic covers the addition of an IP route for a NVMe/TCP director. Addition of an IP route for an iSCSI director is covered in the Create an IP route topic.

## Steps

1. Select a storage system running PowerMaxOS 10 (6079).
2. Select System > iSCSI+NVMe and click the NVME tab to open the NVMe dashboard.
3. Do one of the following: .
   - In the Actions panel, click Create IP Route.
   - Click IP routes and click Create .
4. Select a director from the drop-down menu.
5. Type a value for the IP address.
   You specify the IPv4 address in dotted decimal notation. You specify the IPv6 address in colon-hexadecimal format.
6. Type a value for the Gateway IP.
   You specify an IPv4 or IPv6 address. You specify the IPv4 address in dotted decimal notation. You specify the IPv6 address in colon-hexadecimal format.
7. Type a value for the Prefix.
   You specify an IPv4 prefix length value in the range of 1 through 30. You specify an IPv6 prefix length value in the range of 1 through 128.
8. Type the value for the Network ID.
   Default value is 1. Valid values range from 1 through 16383.
9. Click OK.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com