Jump to main content

# View IP routes

Unisphere provides monitoring and management for Non-Volatile Memory Express (NVMe/TCP) directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system that is running PowerMaxOS 10 (6079).
2. Select System > iSCSI+NVMe and click NVME tab to open the NVMe dashboard.
3. Click IP Routes.

   The following properties display, depending on the operating environment:

   Destination IP | The IPv4 or IPv6 destination IP address of the IP route.
   Prefix | The IPv4 or IPv6 network mask prefix of the IP route.
   Gateway IP | The gateway IP address of the IP route.
   Network ID | The network identity of the IP route.
   Director | The director associated with the IP route.

   To see more information about a NVMe/TCP IP route, select it and click .

   The following parameters are displayed:

   - Destination IP —The IPv4 or IPv6 destination IP address of the IP route
   - Prefix—The IPv4 or IPv6 network mask prefix of the IP route
   - Gateway IP—The gateway IP address of the IP route
   - Network ID—The network identity of the IP route
   - Director—The director with which the IP route is associated.

   The following controls are available, depending on the operating environment:

   - Create— Create an IP route
   - —Delete an IP route

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com