Jump to main content

# 1138

Table 1. SYMAPI_AEVENT2_UID_MOD_SRDFA_SE_TRANS_IDLE,
1138 | SYMAPI_AEVENT2_UID_MOD_SRDFA_SE_TRANS_IDLE,
--- | ---
Category | srdfa session
Component | SRDFA Grp (For example, SRDF-grp=1)
Severity | Info
Message | SRDF/A Session entering transmit idle state.

Table 2. Unisphere policy name
Unisphere policy name | SRDF/A Session entering transmit idle state
--- | ---
Action type | Alert

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com