Jump to main content

# 1210

Table 1. SYMAPI_AEVENT2_UID_ALERT_HOTSPARE_CHANGE
1210 | SYMAPI_AEVENT2_UID_ALERT_HOTSPARE_CHANGE
--- | ---
Category | status
Component | Disk identifier of the Spare, for example:
    Disk=16B:C2 (for Director 16B, DA Interface C, SCSI ID/Target 2)
Severity | For 5x74 and newer arrays: Normal For older arrays: If invoked: Warning If no longer invoked: Normal
Message | For 5x74 and newer arrays: Disk is lo longer a Spare. Disk is now a Spare. Disk is now an invoked Spare. For older arrays: Spare has been invoked against a failed disk. Spare is no longer invoked against a failed disk.

Table 2. Unisphere policy name
Unisphere policy name | Hotspare Invoked
--- | ---
Action type | Alert
Solutions Enabler mapping | This alert is registered as a result of registering for SYMAPI_AEVENT2_UID_ALERT_HOTSPARE_CHANGE

Indicates that a disk has started or stopped acting as a spare.

## Note

With Permanent Sparing on newer arrays, a failing disk and a spare will exchange roles. The failed disk will end up as a failed spare, and the spare will end up as a normal disk. The “Disk is now an invoked Spare” event will rarely if ever be delivered.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com