Jump to main content

# Volume Set Addressing

Volume Set Addressing is an addressing scheme that uses virtual busses, targets, and LUNs to increase greatly the number of LUNs that can be addressed on a target port.

Volume Set Addressing is supported for HP-UX.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com