Jump to main content

# 1205

Table 1. SYMAPI_AEVENT2_UID_ALERT_DEV_CONFIG_CHANGE
1205 | SYMAPI_AEVENT2_UID_ALERT_DEV_CONFIG_CHANGE
--- | ---
Category | status
Component | Device number, for example: Device=1234
Severity | Info
Message | Device configuration has changed.

Table 2. Unisphere policy name
Unisphere policy name | Device Config Change
--- | ---
Action type | Alert/Refresh OM

Indicates that the configuration of some device has changed.

## Notes

- The following aspects of a device's configuration is considered by this event:
  - The base device configuration.
  - The meta configuration of the device (META_HEAD, META_MEMBER).
  - The bound-vs-bound state of a TDEV (bound vs unbound).
  - Whether a dynamic spare disk is invoked for the device.
  - The RDF mode of the device (of either leg for Concurrent SRDF).
  - The data pool bound to by a TDEV changes. This reflects a device being bound, unbound or re-bound to a different pool, and is also triggered when the name of the pool changes.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com