Jump to main content

# 1565

Table 1. SYMAPI_AEVENT2_UID_ALERT_SRP_RELIABILITY_STATE_CHANGE
1556 | SYMAPI_AEVENT2_UID_ALERT_SRP_RELIABILITY_STATE_CHANGE
--- | ---
Category | status
Component | Control window
Severity | Info
Message | Reliability state of an SRP has changed to %s (was: %s)".
     [Optimal|Failed|Degraded-NoSpare|
    Degraded-Rebuilding|Degraded-NoRebuild]

| NOTE: This event is only supported on arrays running PowerMaxOS 6079 or higher.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com