Jump to main content

# 1215

Table 1. SYMAPI_AEVENT2_UID_ALERT_PORT_CONFIG_CHANGE
1215 | SYMAPI_AEVENT2_UID_ALERT_PORT_CONFIG_CHANGE
--- | ---
Category | status
Component | Port, for example:
    Port=SA-03C:2
(for Port 2 on Director SA-03C)
Severity | Info
Message | Port configuration has changed.

Indicates that the configuration changed for a Port on a Front End (FE) Director.

## Notes

- The only aspects of a port's configuration that are considered the following flags from the FA port flags:
- The _VCM_ENABLED flag.
- The _VOL_SET_ADDR (VSA) flag.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com