Jump to main content

# 1052

Table 1. SYMAPI_AEVENT2_UID_MOD_ADAPT_CPY_WRT_PEND
1052 | SYMAPI_AEVENT2_UID_MOD_ADAPT_CPY_WRT_PEND
--- | ---
Category | srdf system
Component | Director (for example, Director=SA-03C)
Severity | Warning
Message | Too many suspend/halt chains encountered, switching to Adaptive Copy Write Pending Mode.

## Note

- System, Mainframe
- Set mode of operation

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com