Jump to main content

# View system front-end director details

Unisphere supports the display of director information.

## Steps

1. Select the storage system.
2. Select System > Hardware.
3. Click the FE Directors tab.
   The Front End Directors list view opens.
4. Select a director and click to open the Front End Director details view.

   The front-end director details view allows you to view and manage a front-end director.

   The following properties display under the Details tab:

   Director | Director name.
   Port | Port.
   Type | Director transmission protocol.
   Director Status | Director status.
   Port Status | Indicates port status: ON or OFF.
   Director Connection Status | Connection status.
   Volumes | Number of volumes that are mapped to the port.
   Mapped Devices (including meta members) | Number of mapped volumes, including any meta members.
   Port ID | Port ID.
   Fibre Channel Loop | Fiber channel loop.
   ACLX | This property indicates whether ACLX is enabled or disabled.
   Common Serial Number | This property indicates whether the Common Serial Number feature is enabled or disabled.
   Unique WWN | This property indicates whether the Unique WWN feature is enabled or disabled.
   Init Point to Point | This property indicates whether Init Point to Point is enabled or disabled.
   Volume Set Addressing | This property indicates whether Volume Set Addressing is enabled or disabled.
   VNX Attached | This property indicates whether VNX Attached is enabled or disabled.
   Avoid Reset Broadcasting | This property indicates whether Avoid Reset Broadcasting feature is enabled or disabled.
   Negotiate Reset | This property indicates whether the Negotiate Reset feature is enabled or disabled. This feature is used for AS/400 systems only (default is off).
   Enable Auto Negotiate | This property indicates whether the Enable Auto Negotiate feature is enabled or disabled.
   Environ Set | This property indicates whether the environmental error reporting feature is enabled or disabled.
   Disable Q Reset on UA | This property indicates whether the Disable Q Reset on UA (Unit Attention) feature is enabled or disabled.
   Soft Reset | This property indicates whether the Soft Reset feature is enabled or disabled for a Bull/GCOS-7 host.
   SCSI 3 | This property indicates whether the SCSI-3 protocol is enabled or disabled. When disabled, the SCSI 2 protocol is supported.
   SCSI Support1(OS2007) | This property indicates whether SCSI Support1 is enabled or disabled.
   No Participating | This property indicates whether the Non Participate feature is enabled or disabled.
   SPC2 Protocol Version | This property indicates whether the SPC Protocol Version feature is enabled or disabled. This feature is used for Windows 2003 environment running Microsoft HCT test version 12.1.
   HP 3000 Mode | This property indicates whether the HP 3000 Mode is enabled or disabled. This feature is used for HP MPE 5.0.
   Sunapee | This property indicates whether the Sunapee feature is enabled or disabled. This feature is used for SUN PDB clusters.
   Siemens | This property indicates whether the Siemens feature is enabled or disabled. This feature is used for Siemens R-series platforms.
   Sequent | This property indicates whether the Sequent feature is enabled or disabled. This feature is used for Sequent platforms.
   Server on AS400 | This property indicates whether the Server of AS400 feature is enabled or disabled. This feature is used For AS/400 platforms.
   Enable AS400 | This property indicates whether Enable AS400 is enabled or disabled.
   OpenVMS | This property indicates whether OpenVMS is enabled or disabled.
   Open Replicator Maximum Ceiling (MB) | Maximum recopy ceiling value.
   Open Replicator Ceiling (%) | Recopy ceiling value.
   Open Replicator Actual Ceiling (MB) | Recopy actual ceiling value.
   Negotiated Speed (GB/Second) | Negotiated speed in GB/Second.

   The Performance panel links you to the performance monitor and analyze views for the director. This panel displays only when the Performance option is installed. Inactive links are displayed if the selected storage system is not registered for data collection.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com