Jump to main content

# Create a NVMe/TCP endpoint

Unisphere provides monitoring and management for Non-Volatile Memory Express (NVMe/TCP) directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system running PowerMaxOS 10 (6079).
2. Select System > iSCSI+NVMe and click NVME tab to open the NVMe dashboard.
3. Do one of the following:
   - From the Actions panel, click Create NVMe/TCP Endpoint.
   - Click NVMe/TCP Endpoints (Attached or Unattached) and click Create.
4. Select a director from the drop-down menu.
5. Type a value for the Network ID.
   Valid values range from 1 through 16383.
6. Type a value for the TCP Port.
   Default value is 4420. Valid values range from 1 through 65535.
7. Optional: Enter a value for the Endpoint Name.
8. Click OK.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com