Jump to main content

# SRDF group SRDF/A flags

SRDF groups provide a collective data transfer path linking volumes of two separate storage systems.

Table 1. SRDF group SRDF/A flag status
Flag | Status
--- | ---
(C) Consistency | X = Enabled; . = Disabled; - = N/A
(S) Status | A = Active; I = Inactive; - = N/A
(R) RDFA Mode | S = Single-session, M = MSC; - = N/A
(M) Msc Cleanup | C = MSC Cleanup required; - = N/A
(T) Transmit Idle | X = Enabled; = Disabled; - = N/A
(D) DSE Status | A = Active; I = Inactive; - = N/A
DSE (A) Autostart | X = Enabled; = Disabled; - = N/A

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com