Jump to main content

# View embedded VASA VP settings details

Unisphere supports the display of embedded VASA VP settings.

## Prerequisites

Embedded applications are installed on the storage system.

## About this task

See Understanding serviceability for an overview of the Unisphere for PowerMax Serviceability functionality.

## Steps

1. Select the storage system.
2. Select Serviceability > Applications > VASA.
3. Select the VP settings tab.
   Select VASA 0 or VASA 1 from the left panel. The following properties display:
   - VP Log File Size(MB)—Select the VP Log File Size from the drop-down list. The default value is 64.
   - VP Log Level—Select error, info (default setting), debug, warning, or trace from the drop-down menu
   - Number of Log Files to be Retained—Select the number of log files to be retained (the range is between 1 and 50). The default value is 25.
   - Maximum Concurrent Connection Per Session—Select a number between 1 and 16. The default value is 16.
   - Retain VP Certificate—Select TRUE (default setting) or FALSE.
   - SYMAPI Debug Log—Select ENABLED or DISABLED (default setting).
4. Click Save to save changes, click Reset to reset the values to their defaults.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com