Jump to main content

# View the iSCSI directors list

Unisphere provides monitoring and management for Internet Small Computer Systems Interface (iSCSI) directors, iSCSI ports, iSCSI endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system that is running HYPERMAX OS 5977 or PowerMaxOS 5978.
2. Select System > iSCSI to open the iSCSI dashboard.
3. Click iSCSI Directors to open the iSCSI Directors list view.
   The following properties display, depending on the operating environment:

   Director | The name of the iSCSI director.
   Ports | The number of iSCSI physical ports associated with the director.
   IP Interfaces | The total number of IP interfaces associated with each physical port on the director.
   Attached iSCSI Endpoints | The total number of unique iSCSI endpoints attached to the IP interfaces associated with the director.
   Unattached iSCSI Endpoints | The total number of unique iSCSI endpoints unattached to the IP interfaces associated with the director.
   IP Routes | The total number of IP routes associated with the director.
   Volumes | The total number of volumes that are mapped to all iSCSI endpoints on that director.

   To see more information about a director, select it and click .

   The following controls are available, depending on the operating environment:

   - Create iSCSI Endpoint— Create an iSCSI endpoint
   - Create IP Route— Create an IP route

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com