Jump to main content

# Understanding initiators

An initiator group is a container of one or more host initiators (Fibre or iSCSI or NVMe/TCP).

Each initiator group can contain up to 64 initiator addresses or 64 child IG names. Initiator groups cannot contain a mixture of host initiators and child IG names.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com