Jump to main content

# 1244

Table 1. SYMAPI_AEVENT2_UID_ALERT_ARR_COMP_STATUS
1244 | SYMAPI_AEVENT2_UID_ALERT_ARR_COMP_STATUS
--- | ---
Category | status
Component | Power=xxx Fan=xxx LCC=xxx Enclosure=xxx MM=xxx IOMC=xxx Dir=xxx
Severity | If Online: Normal If Online Degraded: Warning If Offline: Major If Unknown: Warning
Message | Component state has changed to [Not Present | Unknown | Online | Write Disabled | Offline | Failed]

Table 2. Unisphere policy name
Unisphere policy name | Array Component Events
--- | ---
Action type | Alert

- Online — means that the component is a Normal or Degraded state.
- Online [Degraded] — means that the component is in a degraded state.
- Offline — means that the component is in a Failed state.

The format of the specific component name (xxx above) may differ depending on the VMAX model. Some examples you might encounter are:

Table 3. Components
Component | Description
--- | ---
SB-1/Fan-A | Fan in System Bay
SB-1/ENC-1 | Enclosure within System Bay
SB-1/ENC-1/Fan-A | Fan in Enclosure-Slot within System Bay
SB-1/MIBE-L-2A | MIBE within System Bay
SB-1/MIBE-L-2A/PS-A | Power Supply in MIBE within System Bay

## Notes

Indicates a change in environmental status for one of the following types of sub-components within the VMAX array:

Table 4. Types of subcomponents
Sub-component | Type
--- | ---
Fans: | [ Fan ]
Power Supplies: | [ Power ]
Link Control Cards: | [ LCC ]
Management Modules | [ MM ]
IO Module Carriers | [ IOMC ]
Directors (for environmental alerts): | [ Dir ]
Enclosures or Matrix Interface Board Enclosures | [ Enclosure ]

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com