Jump to main content

# View iSCSI ports details

Unisphere provides monitoring and management for Internet Small Computer Systems Interface (iSCSI) directors, iSCSI ports, iSCSI endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system that is running HYPERMAX OS 5977 or PowerMaxOS 5978.
2. Select System > iSCSI to open the iSCSI dashboard.
3. Click iSCSI Ports to open the iSCSI Ports list view and select a specific director to filter the list.
4. Select a row from the list and click to open the iSCSI Ports details view.

   Properties panel

   The following properties display, depending on the operating environment:

   Director | The name of the director and the iSCSI port combined.
   Status | The status of the iSCSI port (offline or online).
   IP Interfaces | The total number of IP interfaces attached to this iSCSI port.
   Attached iSCSI Endpoints | The list view of iSCSI endpoints on this director that are attached to IP interfaces.
   Volumes | The total number of volumes that are mapped to all iSCSI endpoints on this port.
   Speed GB/Sec | The speed of the iSCSI port.
   IP Interfaces | The list view of IP interfaces that are associated with the physical ports on this director.
   Attached iSCSI Endpoints | The list view of iSCSI endpoints on this director that are attached to IP interfaces.
   Unattached iSCSI Endpoints | The list view of iSCSI endpoints on this director that are unattached.
   Mapped Volumes | The list view of volumes that are mapped to iSCSI endpoints associated with the director.
   iSCSI Director | The list view listing the director that is associated with the selected iSCSI port.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com