Jump to main content

# Unisphere policy name - Alert ID mapping

The following table presents an overview of Unisphere policy names and their corresponding Solutions Enabler Alert or Event IDs. For details on the events, use the hyperlinks.

| NOTE: Hotspare Invoked events and RVA Spare Coverage events are not supported for arrays running PowerMaxOS 10 (6079) and higher.

Table 1. Unisphere policy name - Alert ID mapping
Unisphere policy name | Alert/Event ID | Solutions Enabler event definition
--- | --- | ---
Hotspare Invoked | 1054 | SYMAPI_AEVENT2_UID_MOD_DISKDRV_SPARE_INVK
1060 | SYMAPI_AEVENT2_UID_MOD_RDF_HOTSPARE_INVK
1210 | SYMAPI_AEVENT2_UID_ALERT_HOTSPARE_CHANGE
CG Tripped | 1109 | SYMAPI_AEVENT2_UID_MOD_RDF_CG_TRIG
DB Checksum Triggered | 1108 | SYMAPI_AEVENT2_UID_MOD_DEV_CHKSUM
Port Link Status | 1063 | SYMAPI_AEVENT2_UID_MOD_FCPORT_FAIL
Environmental Alert | 1067 | SYMAPI_AEVENT2_UID_MOD_TEMP_OUT_OF_LIMIT
1150 | SYMAPI_AEVENT2_UID_MOD_LCC_A_TEMP_HIGH
1151 | SYMAPI_AEVENT2_UID_MOD_LCC_B_TEMP_HIGH
SRDF/A Session entering Transmit Idle state | 1138 | SYMAPI_AEVENT2_UID_MOD_SRDFA_SE_TRANS_IDLE
SRDF/A Session recovered from a Transmit Idle state | 1139 | SYMAPI_AEVENT2_UID_MOD_SRDFA_SR_TRANS_IDLE
SRDF/A Session dropped, transit idle state timeout | 1140 | SYMAPI_AEVENT2_UID_MOD_SRDFA_TO_TRANS_IDLE
SRDF/A No Cycle Switch Alert | 1159 | SYMAPI_AEVENT2_UID_ALERT_SRDFA_NO_CYCLE_SWITCH
SRDF Job Flow Control Change | 1160 | SYMAPI_AEVENT2_UID_ALERT_SRDF_JFC_STATE_CHANGE
External disk group fully allocated | 1162 | SYMAPI_AEVENT2_UID_ALERT_EDISK_FULL
Device Status | 1200 | SYMAPI_AEVENT2_UID_ALERT_DEV_STATUS
Director Status | 1202 | SYMAPI_AEVENT2_UID_ALERT_DIRECTOR_STATUS
Port Status | 1203 | SYMAPI_AEVENT2_UID_ALERT_PORT_STATUS
Disk status | 1204 | SYMAPI_AEVENT2_UID_ALERT_DISK_STATUS
Target Enginuity Warning | N/A | N/A. Unisphere for PowerMax generates this alert for each storage system that is not running the minimum suggested Enginuity version.
Thin Device Allocation | 1212 | SYMAPI_AEVENT2_UID_THRESH_TDEV_ALLOCATED
Thin Device Usage | 1213 | SYMAPI_AEVENT2_UID_THRESH_TDEV_USED
Deferred Service Threshold Alert | 1217 | SYMAPI_AEVENT2_UID_ALERT_DFR_SVC_STATE
Array Component Events | 1244 | SYMAPI_AEVENT2_UID_ALERT_ARR_COMP_STATUS
RVA Spare Coverage | 1247 | SYMAPI_AEVENT2_UID_ALERT_DISK_SPARE_CVG
GK Utilization | 1252 | SYMAPI_AEVENT2_UID_BASED_THRESH_GK_UTIL_AVG
GK Timeout | 1253 | SYMAPI_AEVENT2_UID_BASED_GK_TIMEOUT
Storage Resource Pool Free Space | 1512 | SYMAPI_AEVENT2_UID_ALERT_FAST_SRP_ALLOC_CHANGE
Fabric Performance Impact Notification | 1173 | SYMAPI_AEVENT2_UID_MOD_FPIN_NOTIFY
SP Alerts | 1073 | SYMAPI_AEVENT2_UID_MOD_SP_NOT_RESP
1074 | SYMAPI_AEVENT2_UID_MOD_PHONEHOME_FAIL
1082 | SYMAPI_AEVENT2_UID_MOD_PHONEHOME_SUCCESS
1091 | SYMAPI_AEVENT2_UID_MOD_SP_CONNECT_TIME_NOT_FOUND
1092 | SYMAPI_AEVENT2_UID_MOD_SP_COMM_VIA_SERIAL
1093 | SYMAPI_AEVENT2_UID_MOD_REMMGMT_CONNECT
1094 | SYMAPI_AEVENT2_UID_MOD_REMMGMT_REJECT
1095 | SYMAPI_AEVENT2_UID_MOD_REMMGMT_DISCONNECT
1096 | SYMAPI_AEVENT2_UID_ALRM_MEMERR_SP_MEM_ABOVE_LIMIT
1098 | SYMAPI_AEVENT2_UID_MOD_SP_DIR_COMM_ERR
1099 | SYMAPI_AEVENT2_UID_MOD_SP_DIR_QRY_ERR
1100 | SYMAPI_AEVENT2_UID_MOD_SP_COMM_VIA_DIR
1101 | SYMAPI_AEVENT2_UID_MOD_SENSOR_READ_ERR
1102 | SYMAPI_AEVENT2_UID_MOD_SP_CARD_ERR
1104 | SYMAPI_AEVENT2_UID_MOD_SP_DISK_FULL
1107 | SYMAPI_AEVENT2_UID_MOD_PHONEHOME_TRIG
1110 | SYMAPI_AEVENT2_UID_MOD_SP_REBOOTED
SRDF/Metro Automatically Suspended | 1168 | SYMAPI_AEVENT2_UID_MOD_RDF_METRO_SESS_SUSPEND
SRP Reliability State | 1556 | SYMAPI_AEVENT2_UID_ALERT_SRP_RELIABILITY_STATE_CHANGE
Device Config Change | 1205 | SYMAPI_AEVENT2_UID_ALERT_DEV_CONFIG_CHANGE
Event Lost Alert | 2 | SYMAPI_AEVENT2_UID_EVT_EVENTS_LOST
Event Overflow Alert | 3 | SYMAPI_AEVENT2_UID_EVT_EVENTS_OVERFLOW
SRDF Alerts | 1061 | SYMAPI_AEVENT2_UID_MOD_RDF_SIM_MSG
1062 | SYMAPI_AEVENT2_UID_MOD_RDF_ERR
SRDF/A Session | 1112 | SYMAPI_AEVENT2_UID_MOD_RDFA_INACTIVE
1113 | SYMAPI_AEVENT2_UID_MOD_RDFA_ACTIVE
1123 | SYMAPI_AEVENT2_UID_MOD_SESS_DROP_NO_RDF_LNK
1130 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DROP_FROM_HOST
1131 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DROP_PEND_FROM_HOST
1132 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DEACTIV_FROM_HOST
1133 | SYMAPI_AEVENT2_UID_MOD_SRDFA_CONS_DEACTIV_FROM_HOST
1134 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DROP
1135 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DROP_PEND
1158 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DROP_WPL_CP
SRDF/A Auto Recovery Active | 1174 | SYMAPI_AEVENT2_UID_MOD_SRDFA_AUTO_RESTART
SRDF/A Auto Recovery Inactive | 1175 | SYMAPI_AEVENT2_UID_MOD_SRDFA_CONSISTENT
SRDF Link Status | 1064 | SYMAPI_AEVENT2_UID_MOD_RDF_LINKS_DOWN
1065 | SYMAPI_AEVENT2_UID_MOD_RDF_LINKS_UP
1080 | SYMAPI_AEVENT2_UID_MOD_RDF_1LINK_DOWN
1081 | SYMAPI_AEVENT2_UID_MOD_RDF_1LINK_UP
Snapshot Policy Created Snapshot Policy Deleted Snapshot Policy Modified | 1302 | SYMAPI_AEVENT2_UID_ALERT_SNAPSL_CONFIG_CHANGE
Snapshot Policy Added to Storage Group Snapshot Policy Removed from Storage Group | 1336 | SYMAPI_AEVENT2_UID_ALERT_SNAPSL_SG_STATUS_CHANGE
Snapshot Compliance for Storage Group Degraded Snapshot Compliance for Storage Group Improved | N/A | N/A. Unisphere for PowerMax generates this alert.
SRP Effective Used Capacity | 1512 1516 1517 | SYMAPI_AEVENT2_UID_ALERT_FAST_SRP_ALLOC_CHANGE SYMAPI_AEVENT2_UID_ALERT_FAST_SRP_FBA_ALLOC_CHANGE SYMAPI_AEVENT2_UID_ALERT_FAST_SRP_CKD_ALLOC_CHANGE
SRP Effective Capacity Resource Usage | 1570 1571 | SYMAPI_AEVENT2_UID_ALERT_SRP_FBA_EFF_RES_PCT_CHG SYMAPI_AEVENT2_UID_ALERT_SRP_CKD_EFF_RES_PCT_CHG
SRP Over Provisioned Capacity | 1566 1567 | SYMAPI_AEVENT2_UID_ALERT_SRP_FBA_OP_USAGE_PCT_CHG SYMAPI_AEVENT2_UID_ALERT_SRP_CKD_OP_USAGE_PCT_CHG
SRP Physical Capacity | 1568 1569 | SYMAPI_AEVENT2_UID_ALERT_SRP_FBA_PHYSICAL_CAP_CHG SYMAPI_AEVENT2_UID_ALERT_SRP_CKD_PHYSICAL_CAP_CHG
Storage Container Utilization | 1541 | SYMAPI_AEVENT2_UID_ALERT_STOR_CONT_SUBSCR_CAP_CHANGE
Backend Meta Data Usage | 1225 | SYMAPI_AEVENT2_UID_ALERT_BE_METADATAUSE_PCT_CHG
System Meta Data Utilization | 1223 | SYMAPI_AEVENT2_UID_ALERT_SYS_METADATAUSE_PCT_CHG
Local Replication Utilization | 1222 | SYMAPI_AEVENT2_UID_ALERT_LREP_CACHEUSE_PCT_CHG
Frontend Meta Data Usage | 1224 | SYMAPI_AEVENT2_UID_ALERT_FE_METADATAUSE_PCT_CHG
Snapshot SRP Utilization | 1525 | SYMAPI_AEVENT2_UID_ALERT_SG_SNAP_CAP_CHANGE

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com