Jump to main content

# Delete a NVMe/TCP endpoint

Unisphere provides monitoring and management for Non-Volatile Memory Express (NVMe/TCP) directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

## Prerequisites

The NVMe/TCP endpoint must be detached from the IP interface before it can be deleted.

## About this task

Deleting NVMe/TCP endpoints with IP interfaces attached detaches the IP interfaces before deleting the NVMe/TCP endpoint.

The deletion fails if the endpoint is in a port group.

## Steps

1. Select a storage system running PowerMaxOS 10 (6079).
2. Select System > iSCSI+NVMe and click NVME tab to open the NVMe dashboard.
3. Click NVMe/TCP Endpoints (Attached or Unattached).
4. Select an NVMe/TCP endpoint and click .
5. Click OK.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com