Jump to main content

# View NVMe/TCP endpoints

Unisphere provides monitoring and management for Non-Volatile Memory Express (NVMe/TCP) directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

## About this task

To view the NVMe/TCP endpoints:

## Steps

1. Select a storage system that is running PowerMaxOS 10 (6079).
2. Select System > iSCSI+NVMe and click NVME tab to open the NVMe dashboard.
3. Click NVMe/TCP Endpoints (Attached or Unattached).
   The following properties display, depending on the operating environment:

   Dir:Virtual Port | The assigned virtual port for the NVMe/TCP endpoint.
   TCP Port | The TCP port that is to be used for all IP addresses attached to it.
   Name | The custom name value of the NVMe/TCP endpoint.
   Status | The status of the NVMe/TCP endpoint.
   Network ID | The network identity of the IP interface that provides isolated IP routes.
   IP Interfaces | The total number of IP interfaces attached to the NVMe/TCP endpoint.
   NVMe/TCP Ports | The total number of physical IP ports associated with the NVMe/TCP endpoint.
   Volumes | The total number of volumes that are mapped to the NVMe/TCP endpoint.

   To see more information about a NVMe/TCP endpoint, select it and click .

   The following parameters are displayed:

   - Dir:Virtual Port—The assigned virtual port for the NVMe/TCP endpoint
   - TCP Port—The TCP port to be used for all IP addresses attached to it
   - Name—The custom name value of the NVMe/TCP endpoint
   - Status—The status of the NVMe/TCP endpoint
   - Network ID—The network identity of the IP interface that provides isolated IP routes.
   - IP Interfaces—The total number of IP interfaces attached to the NVMe/TCP endpoint.
   - NVMe/TCP Ports—The total number of physical IP ports associated with the NVMe/TCP endpoint.
   - Volumes—The total number of volumes that are mapped to the NVMe/TCP endpoint
   The following controls are available, depending on the operating environment:
   - Create— Create a NVMe/TCP endpoint
   - Attach— Attach an NVMe/TCP endpoint to an IP interface
   - Modify— Modify a NVMe/TCP endpoint
   - Detach— Detach an NVMe/TCP endpoint from an IP interface (only available from the Attached NVMe/TCP Endpoints list view.
   - —Delete a NVMe/TCP endpoint

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com