Jump to main content

# View IP interfaces list

Unisphere provides monitoring and management for Internet Small Computer Systems Interface (iSCSI) directors, iSCSI ports, iSCSI endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system.
2. Select System > iSCSI to open the iSCSI dashboard.
3. Click iSCSI Directors to open the iSCSI Directors list view.
4. Click IP Interfaces to open the IP Interfaces list view and select a specific director to filter the list.
   The following properties display, depending on the operating environment:

   Dir:Port | The combination of the physical director and associated port of the IP interface.
   Network ID | The network identity of the IP interface that provides isolated IP routes.
   IP Address | The destination IPv4 or IPv6 address of the IP interface.
   Prefix | The network mask IPv4 or IPv6 prefix value of the IP interface.
   VLAN ID | The VLAN tag number of the IP interface.
   Dir:Virtual Port | The combination of the physical director and an assigned virtual port or iSCSI endpoint alias of the IP interface.
   Volumes | The total number of volumes mapped to the iSCSI endpoint attached to the IP interface.

   The following controls are available, depending on the operating environment:

   - —View IP interfaces details
   - Create— Create an IP interface
   - Attach— Attach an IP interface to an iSCSI endpoint
   - Detach— Detach an IP interface from an iSCSI endpoint
   - Modify— Edit an IP interface
   - Ping Remote IP— Ping an IP interface
   - —Delete an IP interface

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com