Jump to main content

# Understanding NVMe/TCP

Unisphere provides monitoring and management for NVMe/TCP directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

NVMe/TCP is a NVME-oF technology that supports high performance with lower deployment costs and reduced design complexity. NVMe/TCP defines a new storage networking fabric for the NVMe block storage protocol over a storage networking fabric, and provides the capability of extending NVMe across the entire data center .

The Unisphere UI supports the following operations (on storage systems running PowerMaxOS 10 (6079)):

- View the NVMe dashboard.
- Configure NVMe/TCP using a wizard.
- View NVMe/TCP directors.
- View and configure NVMe/TCP endpoints.
- View NVMe/TCP ports.
- View and configure IP routes.
- View and configure IP interfaces.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com