Jump to main content

# Set the base address

Unisphere supports the setting of the base address.

## About this task

The Set Base Address dialog box is launched from the following locations:

- Provision Storage wizard—The Provision Storage wizard
- CU Image Map wizard—z/OS map from the CU image list view
- Mainframe Volumes Mapping dialog— z/OS map from the volume list view

To set the base address:

## Steps

1. In the Base Address field, specify a new value for the base address.
   Addresses in the range 00-FF are allowed.
2. Click OK.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com