Jump to main content

# Modify an iSCSI endpoint

Unisphere provides monitoring and management for Internet Small Computer Systems Interface (iSCSI) directors, iSCSI ports, iSCSI endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system.
2. Select System > iSCSI to open the iSCSI dashboard.
3. Click iSCSI Endpoints to open the Attached iSCSI Endpoints list view.
4. Select a director and click Modify to open the Modify iSCSI Endpoint dialog.
5. Optional: Type a value for the Endpoint Name.
   If you do not enter a value, the system generates a unique iqn for the endpoint name. If you enter a value, it must follow the following rules:
   - Start with iqn. or eui. strings.
   - Composed of alphanumeric characters, colons, dashes, and periods.
   - Less than, or equal to, 255 characters.
   - Unique on the storage system.
6. Type a value for the Network ID.
   Valid values range from 1 through 16383.
7. Type a value for the TCP Port.
   The default value is 3260. Valid values range from 0 through 65535.
8. Click OK.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com