Jump to main content

# 1233

Table 1. SYMAPI_AEVENT2_UID_ALERT_DYNAMIC_RDF_CONFIG
1233 | SYMAPI_AEVENT2_UID_ALERT_DYNAMIC_RDF_CONFIG
--- | ---
Category | status
Component | -
Severity | Info
Message | Dynamic RDF operation performed on device.

Indicates that a dynamic RDF operation has been performed on some device.

## Note

This is derived from one of the QuickConfig indication maintained on the storage array.

NOTICE: This content was translated using artificial intelligence (AI). It may contain errors and is provided “as is” without any warranty of any kind. To see the original (untranslated) content, please refer to the English version. If you have questions or concerns about this content, please contact Dell at Dell.Translation.Feedback@dell.com