Jump to main content

# SRDF group SRDF/A flags

SRDF groups provide a collective data transfer path linking volumes of two separate storage systems.

Table 1. SRDF group SRDF/A flag status
Flag | Status
--- | ---
(C) Consistency | X = Enabled; . = Disabled; - = N/A
(S) Status | A = Active; I = Inactive; - = N/A
(R) RDFA Mode | S = Single-session, M = MSC; - = N/A
(M) Msc Cleanup | C = MSC Cleanup required; - = N/A
(T) Transmit Idle | X = Enabled; . = Disabled; - = N/A
(D) DSE Status | A = Active; I = Inactive; - = N/A
DSE (A) Autostart | X = Enabled; . = Disabled; - = N/A