Jump to main content

# View the iSCSI directors list

Unisphere provides monitoring and management for Internet Small Computer Systems Interface (iSCSI) directors, iSCSI ports, iSCSI endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system running HYPERMAX OS 5977 or PowerMaxOS 5978.
2. Select System > iSCSI to open the iSCSI dashboard.
3. Click iSCSI Directors to open the iSCSI Directors list view.
   The following properties display, depending on the operating environment:

   Director | The name of the iSCSI director.
   Ports | The number of iSCSI physical ports associated with the director.
   IP Interfaces | The total number of IP interfaces associated with each physical port on the director.
   Attached iSCSI Endpoints | The total number of unique iSCSI endpoints attached to the IP interfaces associated with the director.
   Unattached iSCSI Endpoints | The total number of unique iSCSI endpoints unattached to the IP interfaces associated with the director.
   IP Routes | The total number of IP routes associated with the director.
   Volumes | The total number of volumes that are mapped to all iSCSI endpoints on that director.

   To see more information about a director, select it and click .

   The following controls are available, depending on the operating environment:

   - Create iSCSI Endpoint— Create an iSCSI endpoint
   - Create IP Route— Create an IP route