Jump to main content

# Set Dynamic LUN Addresses

This dialog box is used to manually assign host LUN addresses for a masking operation.

## Steps

1. Select the storage system.
2. Select Hosts > Masking Views.
3. Select a masking view and click Create to open the Create Masking View dialog box.
4. Click Set Dynamic LUNs to open the Set Dynamic LUNs dialog box.

   This dialog box contains the following elements:

   Starting LUN—LUN address that is assigned to the first volume.

   Apply Starting LUN—Sets the address for the volume and keeps the dialog box open for additional operations.

   Next Available LUN—Increments the Starting LUN address to the next available.

   Volumes to be masked—Select the volumes that you want to mask from the volumes list.

   Enter the necessary values and click OK.