Jump to main content

# Set the base address

Unisphere supports the setting of the base address.

## About this task

The Set Base Address dialog box is launched from the following locations:

- Provision Storage wizard—The Provision Storage wizard
- CU Image Map wizard—z/OS map from the CU image list view
- Mainframe Volumes Mapping dialog— z/OS map from the volume list view

To set the base address:

## Steps

1. In the Base Address field, specify a new value for base address.
   Addresses in the range 00-FF are allowed.
2. Click OK.