Jump to main content

# Ping a remote IP interface

Unisphere provides monitoring and management for NVMe/TCP directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system running PowerMaxOS 10 (6079).
2. Select System > iSCSI+NVMe and click the NVME tab to open the NVMe dashboard.
3. Click IP Interfaces.
4. Select an IP interface and click Ping Remote IP.
5. Type the remote IP address.
6. Click OK.