Jump to main content

# View iSCSI ports details

Unisphere provides monitoring and management for Internet Small Computer Systems Interface (iSCSI) directors, iSCSI ports, iSCSI endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system running HYPERMAX OS 5977 or PowerMaxOS 5978.
2. Select System > iSCSI to open the iSCSI dashboard.
3. Click iSCSI Ports to open the iSCSI Ports list view and select a specific director to filter the list.
4. Select a row from the list and click to open the iSCSI Ports details view.

   Properties panel

   The following properties display, depending on the operating environment:

   Director | The name of the director and the iSCSI port combined.
   Status | The status of the iSCSI port (offline or online).
   IP Interfaces | The total number of IP interfaces attached to this iSCSI port.
   Attached iSCSI Endpoints | The list view of iSCSI endpoints on this director that are attached to IP interfaces.
   Volumes | The total number of volumes that are mapped to all iSCSI endpoints on this port.
   Speed GB/Sec | The speed of the iSCSI port.
   IP Interfaces | The list view of IP interfaces that are associated with the physical ports on this director.
   Attached iSCSI Endpoints | The list view of iSCSI endpoints on this director that are attached to IP interfaces.
   Unattached iSCSI Endpoints | The list view of iSCSI endpoints on this director that are unattached.
   Mapped Volumes | The list view of volumes that are mapped to iSCSI endpoints associated with the director.
   iSCSI Director | The list view listing the director that is associated with the selected iSCSI port.