Jump to main content

# Unisphere policy name - Alert ID mapping

The following table presents an overview of Unisphere policy names and their corresponding Solutions Enabler Alert or Event IDs. For details on the events, use the hyperlinks.

| NOTE: Hotspare Invoked events and RVA Spare Coverage events are not supported for arrays running PowerMaxOS 10 (6079) and higher.

Table 1. Unisphere policy name - Alert ID mapping
Unisphere policy name | Alert/Event ID | Solutions Enabler event definition
--- | --- | ---
Hotspare Invoked | 1054 | SYMAPI_AEVENT2_UID_MOD_DISKDRV_SPARE_INVK
1060 | SYMAPI_AEVENT2_UID_MOD_RDF_HOTSPARE_INVK
1210 | SYMAPI_AEVENT2_UID_ALERT_HOTSPARE_CHANGE
CG Tripped | 1109 | SYMAPI_AEVENT2_UID_MOD_RDF_CG_TRIG
DB Checksum Triggered | 1108 | SYMAPI_AEVENT2_UID_MOD_DEV_CHKSUM
Port Link Status | 1063 | SYMAPI_AEVENT2_UID_MOD_FCPORT_FAIL
Environmental Alert | 1067 | SYMAPI_AEVENT2_UID_MOD_TEMP_OUT_OF_LIMIT
1150 | SYMAPI_AEVENT2_UID_MOD_LCC_A_TEMP_HIGH
1151 | SYMAPI_AEVENT2_UID_MOD_LCC_B_TEMP_HIGH
SRDF/A Session entering Transmit Idle state | 1138 | SYMAPI_AEVENT2_UID_MOD_SRDFA_SE_TRANS_IDLE
SRDF/A Session recovered from a Transmit Idle state | 1139 | SYMAPI_AEVENT2_UID_MOD_SRDFA_SR_TRANS_IDLE
SRDF/A Session dropped, transit idle state timeout | 1140 | SYMAPI_AEVENT2_UID_MOD_SRDFA_TO_TRANS_IDLE
SRDF/A No Cycle Switch Alert | 1159 | SYMAPI_AEVENT2_UID_ALERT_SRDFA_NO_CYCLE_SWITCH
SRDF Job Flow Control Change | 1160 | SYMAPI_AEVENT2_UID_ALERT_SRDF_JFC_STATE_CHANGE
External disk group fully allocated | 1162 | SYMAPI_AEVENT2_UID_ALERT_EDISK_FULL
Device Status | 1200 | SYMAPI_AEVENT2_UID_ALERT_DEV_STATUS
Director Status | 1202 | SYMAPI_AEVENT2_UID_ALERT_DIRECTOR_STATUS
Port Status | 1203 | SYMAPI_AEVENT2_UID_ALERT_PORT_STATUS
Disk status | 1204 | SYMAPI_AEVENT2_UID_ALERT_DISK_STATUS
Target Enginuity Warning | N/A | N/A. Unisphere for PowerMax generates this alert for each storage system that is not running the minimum suggested Enginuity version.
Thin Device Allocation | 1212 | SYMAPI_AEVENT2_UID_THRESH_TDEV_ALLOCATED
Thin Device Usage | 1213 | SYMAPI_AEVENT2_UID_THRESH_TDEV_USED
Deferred Service Threshold Alert | 1217 | SYMAPI_AEVENT2_UID_ALERT_DFR_SVC_STATE
Array Component Events | 1244 | SYMAPI_AEVENT2_UID_ALERT_ARR_COMP_STATUS
RVA Spare Coverage | 1247 | SYMAPI_AEVENT2_UID_ALERT_DISK_SPARE_CVG
GK Utilization | 1252 | SYMAPI_AEVENT2_UID_BASED_THRESH_GK_UTIL_AVG
GK Timeout | 1253 | SYMAPI_AEVENT2_UID_BASED_GK_TIMEOUT
Storage Resource Pool Free Space | 1512 | SYMAPI_AEVENT2_UID_ALERT_FAST_SRP_ALLOC_CHANGE
Fabric Performance Impact Notification | 1173 | SYMAPI_AEVENT2_UID_MOD_FPIN_NOTIFY
SP Alerts | 1073 | SYMAPI_AEVENT2_UID_MOD_SP_NOT_RESP
1074 | SYMAPI_AEVENT2_UID_MOD_PHONEHOME_FAIL
1082 | SYMAPI_AEVENT2_UID_MOD_PHONEHOME_SUCCESS
1091 | SYMAPI_AEVENT2_UID_MOD_SP_CONNECT_TIME_NOT_FOUND
1092 | SYMAPI_AEVENT2_UID_MOD_SP_COMM_VIA_SERIAL
1093 | SYMAPI_AEVENT2_UID_MOD_REMMGMT_CONNECT
1094 | SYMAPI_AEVENT2_UID_MOD_REMMGMT_REJECT
1095 | SYMAPI_AEVENT2_UID_MOD_REMMGMT_DISCONNECT
1096 | SYMAPI_AEVENT2_UID_ALRM_MEMERR_SP_MEM_ABOVE_LIMIT
1098 | SYMAPI_AEVENT2_UID_MOD_SP_DIR_COMM_ERR
1099 | SYMAPI_AEVENT2_UID_MOD_SP_DIR_QRY_ERR
1100 | SYMAPI_AEVENT2_UID_MOD_SP_COMM_VIA_DIR
1101 | SYMAPI_AEVENT2_UID_MOD_SENSOR_READ_ERR
1102 | SYMAPI_AEVENT2_UID_MOD_SP_CARD_ERR
1104 | SYMAPI_AEVENT2_UID_MOD_SP_DISK_FULL
1107 | SYMAPI_AEVENT2_UID_MOD_PHONEHOME_TRIG
1110 | SYMAPI_AEVENT2_UID_MOD_SP_REBOOTED
SRDF/Metro Automatically Suspended | 1168 | SYMAPI_AEVENT2_UID_MOD_RDF_METRO_SESS_SUSPEND
SRP Reliability State | 1556 | SYMAPI_AEVENT2_UID_ALERT_SRP_RELIABILITY_STATE_CHANGE
Device Config Change | 1205 | SYMAPI_AEVENT2_UID_ALERT_DEV_CONFIG_CHANGE
Event Lost Alert | 2 | SYMAPI_AEVENT2_UID_EVT_EVENTS_LOST
Event Overflow Alert | 3 | SYMAPI_AEVENT2_UID_EVT_EVENTS_OVERFLOW
SRDF Alerts | 1061 | SYMAPI_AEVENT2_UID_MOD_RDF_SIM_MSG
1062 | SYMAPI_AEVENT2_UID_MOD_RDF_ERR
SRDF/A Session | 1112 | SYMAPI_AEVENT2_UID_MOD_RDFA_INACTIVE
1113 | SYMAPI_AEVENT2_UID_MOD_RDFA_ACTIVE
1123 | SYMAPI_AEVENT2_UID_MOD_SESS_DROP_NO_RDF_LNK
1130 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DROP_FROM_HOST
1131 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DROP_PEND_FROM_HOST
1132 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DEACTIV_FROM_HOST
1133 | SYMAPI_AEVENT2_UID_MOD_SRDFA_CONS_DEACTIV_FROM_HOST
1134 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DROP
1135 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DROP_PEND
1158 | SYMAPI_AEVENT2_UID_MOD_SRDFA_DROP_WPL_CP
SRDF/A Auto Recovery Active | 1174 | SYMAPI_AEVENT2_UID_MOD_SRDFA_AUTO_RESTART
SRDF/A Auto Recovery Inactive | 1175 | SYMAPI_AEVENT2_UID_MOD_SRDFA_CONSISTENT
SRDF Link Status | 1064 | SYMAPI_AEVENT2_UID_MOD_RDF_LINKS_DOWN
1065 | SYMAPI_AEVENT2_UID_MOD_RDF_LINKS_UP
1080 | SYMAPI_AEVENT2_UID_MOD_RDF_1LINK_DOWN
1081 | SYMAPI_AEVENT2_UID_MOD_RDF_1LINK_UP
Snapshot Policy Created Snapshot Policy Deleted Snapshot Policy Modified | 1302 | SYMAPI_AEVENT2_UID_ALERT_SNAPSL_CONFIG_CHANGE
Snapshot Policy Added to Storage Group Snapshot Policy Removed from Storage Group | 1336 | SYMAPI_AEVENT2_UID_ALERT_SNAPSL_SG_STATUS_CHANGE
Snapshot Compliance for Storage Group Degraded Snapshot Compliance for Storage Group Improved | N/A | N/A. Unisphere for PowerMax generates this alert.
SRP Effective Used Capacity | N/A | SYMAPI_AEVENT2_UID_ALERT_FAST_SRP_ALLOC_CHANGE SYMAPI_AEVENT2_UID_ALERT_FAST_SRP_FBA_ALLOC_CHANGE SYMAPI_AEVENT2_UID_ALERT_FAST_SRP_CKD_ALLOC_CHANGE
SRP Effective Capacity Resource Usage | 1570 1571 | SYMAPI_AEVENT2_UID_ALERT_SRP_FBA_EFF_RES_PCT_CHG SYMAPI_AEVENT2_UID_ALERT_SRP_CKD_EFF_RES_PCT_CHG
SRP Over Provisioned Capacity | 1566 1567 | SYMAPI_AEVENT2_UID_ALERT_SRP_FBA_OP_USAGE_PCT_CHG SYMAPI_AEVENT2_UID_ALERT_SRP_CKD_OP_USAGE_PCT_CHG
SRP Physical Capacity | 1568 1569 | SYMAPI_AEVENT2_UID_ALERT_SRP_FBA_PHYSICAL_CAP_CHG SYMAPI_AEVENT2_UID_ALERT_SRP_CKD_PHYSICAL_CAP_CHG
Storage Container Utilization | 1541 | SYMAPI_AEVENT2_UID_ALERT_STOR_CONT_SUBSCR_CAP_CHANGE
Backend Meta Data Usage | 1225 | SYMAPI_AEVENT2_UID_ALERT_BE_METADATAUSE_PCT_CHG
System Meta Data Utilization | 1223 | SYMAPI_AEVENT2_UID_ALERT_SYS_METADATAUSE_PCT_CHG
Local Replication Utilization | 1222 | SYMAPI_AEVENT2_UID_ALERT_LREP_CACHEUSE_PCT_CHG
Frontend Meta Data Usage | 1224 | SYMAPI_AEVENT2_UID_ALERT_FE_METADATAUSE_PCT_CHG
Snapshot SRP Utilization | 1525 | SYMAPI_AEVENT2_UID_ALERT_SG_SNAP_CAP_CHANGE