Jump to main content

# Delete an IP interface

Unisphere provides monitoring and management for NVMe/TCP directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

## Prerequisites

The IP interface must be detached from the NVMe/TCP endpoint in order to delete it.

## Steps

1. Select a storage system running PowerMaxOS 10 (6079).
2. Select System > iSCSI+NVMe and click the NVME tab to open the NVMe dashboard.
3. Click IP Interfaces.
4. Select an IP interface and click .
5. Click OK.