Jump to main content

# Modify an iSCSI endpoint

Unisphere provides monitoring and management for Internet Small Computer Systems Interface (iSCSI) directors, iSCSI ports, iSCSI endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system.
2. Select System > iSCSI to open the iSCSI dashboard.
3. Click iSCSI Endpoints to open the Attached iSCSI Endpoints list view.
4. Select a director and click Modify to open the Modify iSCSI Endpoint dialog.
5. Optional: Type a value for the Endpoint Name.
   If you do not enter a value, the system generates a unique iqn for the endpoint name. If you enter a value, it must follow the following rules:
   - Start with iqn. or eui. strings.
   - Be composed of alphanumeric characters, colons, dashes, and periods.
   - Be less than, or equal to, 255 characters.
   - Be unique on the storage system.
6. Type a value for the Network ID.
   Valid values range from 1 through 16383.
7. Type a value for the TCP Port.
   Default value is 3260. Valid values range from 0 through 65535.
8. Click OK.