Jump to main content

# Enable an iSCSI endpoint

Unisphere provides monitoring and management for Internet Small Computer Systems Interface (iSCSI) directors, iSCSI ports, iSCSI endpoints, IP interfaces, and IP routes.

## Prerequisites

The enable operation does not apply for unattached iSCSI endpoints associated with storage systems running PowerMaxOS 10 (6079).

## Steps

1. Select a storage system.
2. Select System > iSCSI to open the iSCSI dashboard.
3. Click iSCSI Endpoints to open the (Attached or Unattached) iSCSI endpoints list view.
4. Select an iSCSI endpoint and click Enable.
5. Click OK.