Jump to main content

# View the NVMe/TCP directors

Unisphere provides monitoring and management for Non-Volatile Memory Express (NVMe/TCP) directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

## About this task

To view the NVMe/TCP directors:

## Steps

1. Select a storage system running PowerMaxOS 10 (6079).
2. Select System > iSCSI+NVMe and click NVME tab to open the NVMe dashboard.
3. Click NVMe/TCP Directors to open the NVMe/TCP Directors list view.
   The following properties display, depending on the operating environment:

   Director | The name of the NVMe/TCP director.
   Ports | The number of NVMe/TCP physical ports associated with the director.
   IP Interfaces | The total number of IP interfaces associated with each physical port on the director.
   Attached NVMe/TCP Endpoints | The total number of unique NVMe/TCP endpoints attached to the IP interfaces associated with the director.
   Unattached NVMe/TCP Endpoints | The total number of unique NVMe/TCP endpoints unattached to the IP interfaces associated with the director.
   IP Routes | The total number of IP routes associated with the director.
   Volumes | The total number of volumes that are mapped to all NVMe/TCP endpoints on that director.

   To see more information about a director, select it and click .

   The following parameters are displayed:

   - NVMe/TCP Ports—The number of NVMe/TCP physical ports associated with the director
   - IP Interfaces—The total number of IP interfaces associated with each physical port on the director.
   - Attached NVMe/TCP Endpoints—The total number of unique NVMe/TCP endpoints attached to the IP interfaces associated with the director.
   - Unattached NVMe/TCP Endpoints—The total number of unique NVMe/TCP endpoints unattached to the IP interfaces associated with the director.
   - IP Routes—The total number of IP routes associated with the director.
   - Volumes—The total number of volumes that are mapped to all NVMe/TCP endpoints on that director

   The following controls are available, depending on the operating environment:

   - Create NVMe/TCP Endpoint— Create a NVMe/TCP endpoint
   - Create IP Route— Create an IP route