Jump to main content

# Create a NVMe/TCP endpoint

Unisphere provides monitoring and management for Non-Volatile Memory Express (NVMe/TCP) directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system running PowerMaxOS 10 (6079).
2. Select System > iSCSI+NVMe and click NVME tab to open the NVMe dashboard.
3. Do one of the following:
   - From the Actions panel, click Create NVMe/TCP Endpoint.
   - Click NVMe/TCP Endpoints (Attached or Unattached) and click Create.
4. Select a director from the drop-down menu.
5. Type a value for the Network ID.
   Valid values range from 1 through 16383.
6. Type a value for the TCP Port.
   Default value is 4420. Valid values range from 1 through 65535.
7. Optional: Enter a value for the Endpoint Name.
8. Click OK.