Jump to main content

# 1565

Table 1. SYMAPI_AEVENT2_UID_ALERT_SRP_RELIABILITY_STATE_CHANGE
1556 | SYMAPI_AEVENT2_UID_ALERT_SRP_RELIABILITY_STATE_CHANGE
--- | ---
Category | status
Component | Control window
Severity | Info
Message | Reliability state of an SRP has changed to %s (was: %s)".
     [Optimal|Failed|Degraded-NoSpare|
    Degraded-Rebuilding|Degraded-NoRebuild]

| NOTE: This event is only supported on arrays running PowerMaxOS 6079 or higher.