Jump to main content

# View system front-end director details

Unisphere supports the display of director information.

## Steps

1. Select the storage system.
2. Select System > Hardware.
3. Click the FE Directors tab.
   The Front End Directors list view opens.
4. Select a director and click to open the Front End Director details view.

   The front-end director details view allows you to view and manage a front-end director.

   The following properties display under the Details tab:

   Director | Director name.
   Port | Port.
   Type | Director transmission protocol.
   Director Status | Director status.
   Port Status | Indicates port status: ON or OFF.
   Director Connection Status | Connection status.
   Volumes | Number of volumes that are mapped to the port.
   Mapped Devices (including meta members) | Number of mapped volumes, including any meta members.
   Port ID | Port ID.
   Fibre Channel Loop | Fibre channel loop.
   ACLX | Indicates whether ACLX is enabled or disabled.
   Common Serial Number | Indicates whether Common Serial Number feature is enabled or disabled.
   Unique WWN | Indicates whether Unique WWN feature is enabled or disabled.
   Init Point to Point | Indicates whether Init Point to Point is enabled or disabled.
   Volume Set Addressing | Indicates whether Volume Vet Addressing is enabled or disabled.
   VNX Attached | Indicates whether VNX Attached is enabled or disabled.
   Avoid Reset Broadcasting | Indicates whether Avoid Reset Broadcasting feature is enabled or disabled.
   Negotiate Reset | Indicates whether Negotiate Reset feature is enabled or disabled. This feature is used for AS/400 systems only (default is off).
   Enable Auto Negotiate | Indicates whether Enable Auto Negotiate feature is enabled or disabled.
   Environ Set | Indicates whether environmental error reporting feature is enabled or disabled.
   Disable Q Reset on UA | Indicates whether the Disable Q Reset on UA (Unit Attention) is enabled or disabled.
   Soft Reset | Indicates whether Soft Reset feature is enabled or disabled for a Bull/GCOS-7 host.
   SCSI 3 | Indicates whether SCSI-3 protocol is enabled or disabled. When disabled, the SCSI 2 protocol is supported.
   SCSI Support1(OS2007) | Indicates whether SCSI Support1 is enabled or disabled.
   No Participating | Indicates whether Non Participate feature is enabled or disabled.
   SPC2 Protocol Version | Indicates whether SPC Protocol Version feature is enabled or disabled. This feature is used for Windows 2003 environment running Microsoft HCT test version 12.1.
   HP 3000 Mode | Indicates whether HP 3000 Mode is enabled or disabled. This feature is used for HP MPE 5.0.
   Sunapee | Indicates whether Sunapee feature is enabled or disabled. This feature is used for SUN PDB clusters.
   Siemens | Indicates whether Siemens feature is enabled or disabled. This feature is used for Siemens R-series platforms.
   Sequent | Indicates whether the Sequent feature is enabled or disabled. This feature is used for Sequent platforms.
   Server on AS400 | Indicates whether Server of AS400 feature is enabled or disabled. This feature is used For AS/400 platforms.
   Enable AS400 | Indicates whether Enable AS400 is enabled or disabled.
   OpenVMS | Indicates whether OpenVMS is enabled or disabled.
   Open Replicator Maximum Ceiling (MB) | Maximum recopy ceiling value.
   Open Replicator Ceiling (%) | Recopy ceiling value.
   Open Replicator Actual Ceiling (MB) | Recopy actual ceiling value.
   Negotiated Speed (GB/Second) | Negotiated speed in GB/Second.

   The Performance panel links you to the performance monitor and analyze views for the director. This panel displays only when the Performance option is installed. Inactive links are displayed if the selected storage system is not registered for data collection.