Jump to main content

# Detach an IP interface from an iSCSI endpoint

Unisphere provides monitoring and management for Internet Small Computer Systems Interface (iSCSI) directors, iSCSI ports, iSCSI endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system.
2. Select System > iSCSI to open the iSCSI dashboard.
3. Click IP Interfaces to open the IP Interfaces list view.
4. Select an IP interface and click Detach.
5. Click OK.