Jump to main content

# Modify a NVMe/TCP endpoint

Unisphere provides monitoring and management for Non-Volatile Memory Express (NVMe/TCP) directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system running PowerMaxOS 10 (6079).
2. Select System > iSCSI+NVMe and click NVME tab to open the NVMe dashboard.
3. Select a director and click Modify.
4. Modify the value for the Network ID.
   Valid values range from 1 through 16383.
5. Modify the value for the TCP Port.
   Default value is 4420. Valid values range from 1 through 65535.
6. Modify the value for the Endpoint Name.
7. Click OK.