Jump to main content

# View NVMe/TCP endpoints

Unisphere provides monitoring and management for Non-Volatile Memory Express (NVMe/TCP) directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

## About this task

To view the NVMe/TCP endpoints:

## Steps

1. Select a storage system running PowerMaxOS 10 (6079).
2. Select System > iSCSI+NVMe and click NVME tab to open the NVMe dashboard.
3. Click NVMe/TCP Endpoints (Attached or Unattached).
   The following properties display, depending on the operating environment:

   Dir:Virtual Port | The assigned virtual port for the NVMe/TCP endpoint.
   TCP Port | The TCP port to be used for all IP addresses attached to it.
   Name | The custom name value of the NVMe/TCP endpoint.
   Status | The status of the NVMe/TCP endpoint.
   Network ID | The network identity of the IP interface that provides isolated IP routes.
   IP Interfaces | The total number of IP interfaces attached to the NVMe/TCP endpoint.
   NVMe/TCP Ports | The total number of physical IP ports associated with the NVMe/TCP endpoint.
   Volumes | The total number of volumes that are mapped to the NVMe/TCP endpoint.

   To see more information about a NVMe/TCP endpoint, select it and click .

   The following parameters are displayed:

   - Dir:Virtual Port—The assigned virtual port for the NVMe/TCP endpoint
   - TCP Port—The TCP port to be used for all IP addresses attached to it
   - Name—The custom name value of the NVMe/TCP endpoint
   - Status—The status of the NVMe/TCP endpoint
   - Network ID—The network identity of the IP interface that provides isolated IP routes.
   - IP Interfaces—The total number of IP interfaces attached to the NVMe/TCP endpoint.
   - NVMe/TCP Ports—The total number of physical IP ports associated with the NVMe/TCP endpoint.
   - Volumes—The total number of volumes that are mapped to the NVMe/TCP endpoint
   The following controls are available, depending on the operating environment:
   - Create— Create a NVMe/TCP endpoint
   - Attach— Attach an NVMe/TCP endpoint to an IP interface
   - Modify— Modify a NVMe/TCP endpoint
   - Detach— Detach an NVMe/TCP endpoint from an IP interface (only available from the Attached NVMe/TCP Endpoints list view.
   - —Delete a NVMe/TCP endpoint