Jump to main content

# 1233

Table 1. SYMAPI_AEVENT2_UID_ALERT_DYNAMIC_RDF_CONFIG
1233 | SYMAPI_AEVENT2_UID_ALERT_DYNAMIC_RDF_CONFIG
--- | ---
Category | status
Component | -
Severity | Info
Message | Dynamic RDF operation performed on device.

Indicates that a dynamic RDF operation has been performed on some device.

## Note

This is derived from one of the QuickConfig indication maintained on the storage array.