Jump to main content

# FICON Emulation Threads metrics

Unisphere collects and displays metrics for FICON emulation threads.

Within the PM metrics section, V4 is used to denote that the metric is supported only by a storage system (array) running PowerMaxOS 10 (6079). V3 is used to denote that the metric is supported only by a storage system (array) running HYPERMAX OS 5977 or PowerMaxOS 5978. Metrics without the denotation are supported by all storage systems (arrays).

The following table lists all metrics that are available for FICON emulation threads.

Table 1. FICON emulation threads metrics
Metric | Description
--- | ---
% Busy | The percentage of time the FICON emulation threads were busy
% Idle | The percentage of time the FICON emulation threads were idle