Jump to main content

# View IP interfaces list

Unisphere provides monitoring and management for Internet Small Computer Systems Interface (iSCSI) directors, iSCSI ports, iSCSI endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system.
2. Select System > iSCSI to open the iSCSI dashboard.
3. Click iSCSI Directors to open the iSCSI Directors list view.
4. Click IP Interfaces to open the IP Interfaces list view and select a specific director to filter the list.
   The following properties display, depending on the operating environment:

   Dir:Port | The combination of the physical director and associated port of the IP interface.
   Network ID | The network identity of the IP interface that provides isolated IP routes.
   IP Address | The destination IPv4 or IPv6 address of the IP interface.
   Prefix | The network mask IPv4 or IPv6 prefix value of the IP interface.
   VLAN ID | The VLAN tag number of the IP interface.
   Dir:Virtual Port | The combination of the physical director and assigned virtual port or iSCSI endpoint alias of the IP interface.
   Volumes | The total number of volumes mapped to the iSCSI endpoint attached to the IP interface.

   The following controls are available, depending on the operating environment:

   - —View IP interfaces details
   - Create— Create an IP interface
   - Attach— Attach an IP interface to an iSCSI endpoint
   - Detach— Detach an IP interface from an iSCSI endpoint
   - Modify— Edit an IP interface
   - Ping Remote IP— Ping an IP interface
   - —Delete an IP interface