Jump to main content

# 1244

Table 1. SYMAPI_AEVENT2_UID_ALERT_ARR_COMP_STATUS
1244 | SYMAPI_AEVENT2_UID_ALERT_ARR_COMP_STATUS
--- | ---
Category | status
Component | Power=xxx Fan=xxx LCC=xxx Enclosure=xxx MM=xxx IOMC=xxx Dir=xxx
Severity | If Online: Normal If Online Degraded: Warning If Offline: Major If Unknown: Warning
Message | Component state has changed to [Not Present | Unknown | Online | Write Disabled | Offline | Failed]

Table 2. Unisphere policy name
Unisphere policy name | Array Component Events
--- | ---
Action type | Alert

- Online — means that the component is a Normal or Degraded state.
- Online [Degraded] — means that the component is in a degraded state.
- Offline — means that the component is in a Failed state.

The format of the specific component name (xxx above) may differ depending on the VMAX model. Some examples you might encounter are:

Table 3. Components
Component | Description
--- | ---
SB-1/Fan-A | Fan in System Bay
SB-1/ENC-1 | Enclosure within System Bay
SB-1/ENC-1/Fan-A | Fan in Enclosure-Slot within System Bay
SB-1/MIBE-L-2A | MIBE within System Bay
SB-1/MIBE-L-2A/PS-A | Power Supply in MIBE within System Bay

## Notes

Indicates a change in environmental status for one of the following types of sub-components within the VMAX array:

Table 4. Types of subcomponents
Sub-component | Type
--- | ---
Fans: | [ Fan ]
Power Supplies: | [ Power ]
Link Control Cards: | [ LCC ]
Management Modules | [ MM ]
IO Module Carriers | [ IOMC ]
Directors (for environmental alerts): | [ Dir ]
Enclosures or Matrix Interface Board Enclosures | [ Enclosure ]