Jump to main content

# Create an IP route

Unisphere provides monitoring and management for Internet Small Computer Systems Interface (iSCSI) directors, iSCSI ports, iSCSI endpoints, IP interfaces, and IP routes.

## About this task

This topic covers the addition of an IP route for an iSCSI director. Addition of an IP route for a NVMe/TCP director is covered in the Create an IP route topic.

## Steps

1. Select a storage system.
2. Select System > iSCSI to open the iSCSI dashboard.
3. In the Actions panel, click Create IP Route.
4. Select a director from the drop-down menu.
5. Type a value for the Gateway IP.
   You specify an IPv4 or IPv6 address. You specify the IPv4 address in dotted decimal notation. You specify the IPv6 address in colon-hexadecimal format.
6. Type a value for the Destination IP.
   You specify the IPv4 address in dotted decimal notation. You specify the IPv6 address in colon-hexadecimal format.
7. Type a value for the Prefix.
   You specify an IPv4 prefix length value in the range of 1 through 30. You specify an IPv6 prefix length value in the range of 1 through 128.
8. Optional: Type the value for the Network ID.
   Default value is 1. Valid values range from 1 through 16383.
9. Click OK.