Jump to main content

# View NVMe/TCP ports

Unisphere provides monitoring and management for Non-Volatile Memory Express (NVMe/TCP) directors, NVMe/TCP ports, NVMe/TCP endpoints, IP interfaces, and IP routes.

## Steps

1. Select a storage system running PowerMaxOS 10 (6079).
2. Select System > iSCSI+NVMe and click NVME tab to open the NVMe dashboard.
3. Click NVMe/TCP Ports to open the NVMe/TCP Ports list view and select a specific director to filter the list.
   The following properties display, depending on the operating environment:

   Director | The name of the NVMe/TCP director.
   Port | The NVMe/TCP physical port number associated with the director.
   Status | The status of the physical port (offline or online).
   IP Interfaces | The total number of IP interfaces associated with the physical port.
   NVMe/TCP Endpoints | The number of NVMe/TCP endpoints that are attached to the IP interfaces.
   Volumes | The total number of volumes that are mapped to all NVMe/TCP endpoints on that port.

   To see more information about a NVMe/TCP port, select it and click .

   The following parameters are displayed:
   - Director—The name of the NVMe/TCP director
   - Status—The status of the physical port (offline or online)
   - IP Interfaces—The total number of IP interfaces that are associated with the physical port
   - Attached NVMe/TCP Endpoints—The number of NVMe/TCP endpoints that are attached to the IP interfaces
   - Volumes—The total number of volumes that are mapped to all NVMe/TCP endpoints on that port
   - Speed GB/Sec—The port speed (in GB per seconds)
   The following controls are available, depending on the operating environment:
   - Create IP Interface— Create an IP interface