Jump to main content

# View SRDF director IP Interfaces

Unisphere supports the display of SRDF director IP interfaces.

## Steps

1. Select the storage system.
2. Select System > Hardware.
3. Click the RDF Directors tab.
4. Select a director from the RDF Directors list and click to open its details view.
5. Click the number in the IP Interface field.
   Use the IP Interface list to view the IP interfaces mapped to the RE director. The following properties display, depending on the operating environment:

   Dir:Port | The combination of the physical director and associated port of the IP interface.
   IP Address | The destination IPv4 or IPv6 address of the IP interface.
   Prefix | The network mask IPv4 or IPv6 prefix value of the IP interface.
   Default Gateway | The default gateway.
   MTU | Maximum Transmission Unit

   The following controls are available, depending on the operating environment:
   - Create— Create an IP interface
   - Modify— Edit an IP interface
   - Ping Remote IP— Ping an IP interface
   - —Delete an IP interface